{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ALTERAÇÃO"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ALTERAÇÃO","index":0,"n_rows":2,"n_cols":7,"rows_kept":2,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["#Proc","SDIC","NCM Publicado","Descrição Publicada em Resolução CAMEX ","Resolução que concedeu o Ex-tarifário","NCM proposto","Descrição proposta"]
[14428,"X4-12A","8412.21.90","Ex 068 - Motores Hidráulicos de pistões axiais de deslocamento volumétrico de 45,3 cm3/revolução, pressão máxima de 420 kgf/cm2, vazão máxima até 143,8 l/min, rotação máxima de 3100 rpm, conjugado a um redutor planetário com relação de transmissão de 24,58 , torque do conjunto até 4,53 kN.m, para sistema de giro de máquinas autopropulsadas.","Resolução Camex nº 24, de 30/12/2019","8483.40.10","Redutores Planetários para ser conjugado a motor hidráulico de pistões axiais, com relação de transmissão de 24,58, para sistema de giro de máquinas autopropulsadas."]