{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tabela de preços unitários"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabela de preços unitários","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[[30,1,30,7],[3,0,3,3],[4,0,4,3],[0,0,1,7],[2,0,2,7],[3,4,3,7],[4,4,4,7],[6,1,6,7],[19,1,19,7]],"flags":["formulas_cached_only"]}
["MODELO PARA APRESENTAÇÃO DOS VALORES DOS ITENS \nAPRESENTADOS NO PLANO DE TRABALHO "]
[]
["Modelo para apresentação dos valores dos itens apresentados no Plano de Trabalho (extrair SOMENTE da Tabela SINAPI online - CEF)                                                                                                                                                                                                                                    Planilha de preços unitários, que use como referência os preços praticados pelo SINAPI - Sistema Nacional de Pesquisa de Custos e índices da Construção Civil, da Caixa Econômica Federal, inclusive BDI."]
["Informar nº da Tabela de Referência: SINAPI 07/2019 - com desoneração",null,null,null," Exemplo do cálculo item 1.1: 0,36+25% = 0,09 = 0,45*2.400 = 1.080,00"]
["BDI - informar a porcentagem: 25%",null,null,null,"Composição e 10,5% - insumos"]
["ITEM","CÓDIGO SINAPI","ESPECIFICAÇÃO","UNIDADE","QUANTIDADE","PREÇOS SEM BDI","CASO POSSUA PREÇOS COM BDI","TOTAL"]
[1,"SERVIÇOS PRELIMINARES"]
["1.1",78472,"Locação da obra-serviços topográficos","M²",2400,0.36,0.45,1080]
["1.2","73822/2","Limpeza dcj terreno com equipamento mecanizado","M²",2400,0.49,"R$                         -   ",0]
["1.3",74209,"Placa de obra 1,25 m x 2,0 m","M²",2.5,0,429.84,0]
["1.4"]
["1.5"]
["1.6"]
["1.7"]
["1.8"]
["1.9"]
["1.10"]
["1.11"]
["1.12"]
[2,"PISO-GRAMA SINTÉTICA"]
["2.1",93355,"Escavação manual ate l,0 m","M³",60.8,52.69,0,0]
["2.2",83664,"Dreno #20t:m","M",304,0,75.28,0]
["2.3","73883/2","Brita leito grama 20cm com pó de pedra","M³",30.4,0,128.35,0]
["2.4"]
["2.5"]
["2.6"]
["2.7"]
["2.8"]
["2.9"]
["2.10"]
[3,"ALAMBRADO 6 EQUIPAMENTO"]
["3.1","73787/1","Alambrado em tubo aço galvanizado;tela arame ver PVC","M²",420,176.47,0,0]
["3.2",94970,"Concreto fck 2t)Mpa","M³",3.15,35.41,0,0]
["3.3","74157/4","Lançamento concreto fck 20Mpa","M³",3.15,0,111.16,0]
["3.4"]
["3.5"]
["3.6"]
["3.7"]
["3.8"]
["3.9"]
["3.10"]