{"text_format":"2","workbook":"xls","n_sheets":9,"sheets":["Tabela I.1","Gráf I1 Capacidade Instalada EE","Tabela I.1.1","Tabela I.2","Tabela I.3","Gráf I.2 Cap Instalada Refino","aux I.1","auxI.2","auxI.3"],"not_rendered":{"charts":6,"images":3,"macros":0,"external_links":2,"defined_names":4,"comments":3,"pivot_tables":0},"unopened":[{"sheet":"Gráf I1 Capacidade Instalada EE","index":1,"reason":"not_a_worksheet"},{"sheet":"Gráf I.2 Cap Instalada Refino","index":5,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabela I.1","index":0,"n_rows":61,"n_cols":17,"rows_kept":61,"cut":false,"hidden":false,"merged":[[4,1,4,3],[4,14,4,16],[5,14,5,16],[4,4,4,6],[5,4,5,6],[4,7,4,9],[5,7,5,9],[5,1,5,3],[4,10,4,12]],"flags":["formulas_cached_only"]}
["Anexo I. Capacidade Instalada - Brasil"]
[]
["Tabela I.1 Capacidade Instalada de Geração Elétrica"]
["Table I.1 Installed Capacity of Electricity Generation  ",{"$nulls":15},"MW"]
[null,"HIDRO1",null,null,"TERMO",null,null,"EÓLICA",null,null,"SOLAR4",null,null,"NUCLEAR","TOTAL"]
["                      HYDRO (1)","                 HYDRO ",null,null,"                 THERMO",null,null,"WIND",null,null,null,"SOLAR4",null,"NUCLEAR","TOTAL"]
[null,"SP / PIE ²","APE ³","TOTAL","SP e/ou PIE","APE","TOTAL","SP e/ou PIE","APE","TOTAL","SP e/ou PIE","APE","TOTAL","SP e/ou PIE","SP e/ou PIE","APE","TOTAL"]
[1974,13224,500,13724,2489,1920,4409,0,0,0,null,null,null,0,15713,2420,18133]
[1975,15815,501,16316,2436,2216,4652,0,0,0,null,null,null,0,18251,2717,20968]
[1976,17343,561,17904,2457,2223,4680,0,0,0,null,null,null,0,19800,2784,22584]
[1977,18835,561,19396,2729,2214,4943,0,0,0,null,null,null,0,21564,2775,24339]
[1978,21104,561,21665,3048,2259,5307,0,0,0,null,null,null,0,24152,2820,26972]
[1979,23667,568,24235,3573,2411,5984,0,0,0,null,null,null,0,27240,2979,30219]
[1980,27081,568,27649,3484,2339,5823,0,0,0,null,null,null,0,30565,2907,33472]
[1981,30596,577,31173,3655,2441,6096,0,0,0,null,null,null,0,34251,3018,37269]
[1982,32542,614,33156,3687,2503,6190,0,0,0,null,null,null,0,36229,3117,39346]
[1983,33556,622,34178,3641,2547,6188,0,0,0,null,null,null,0,37197,3169,40366]
[1984,34301,622,34923,3626,2547,6173,0,0,0,null,null,null,0,37927,3169,41096]
[1985,36453,624,37077,3708,2665,6373,0,0,0,null,null,null,657,40818,3289,44107]
[1986,37162,624,37786,3845,2665,6510,0,0,0,null,null,null,657,41664,3289,44953]
[1987,39693,636,40329,3910,2665,6575,0,0,0,null,null,null,657,44260,3301,47561]
[1988,41583,645,42228,4025,2665,6690,0,0,0,null,null,null,657,46265,3310,49575]
[1989,44172,624,44796,4007,2665,6672,0,0,0,null,null,null,657,48836,3289,52125]
[1990,44934,624,45558,4170,2665,6835,0,0,0,null,null,null,657,49761,3289,53050]
[1991,45992,624,46616,4203,2665,6868,0,0,0,null,null,null,657,50852,3289,54141]
[1992,47085,624,47709,4018.5,2665,6683.5,0.075,0,0.075,null,null,null,657,51760.575,3289,55049.575]
[1993,47967,624,48591,4127.5,2847,6974.5,0.075,0,0.075,null,null,null,657,52751.575,3471,56222.575]
[1994,49297,624,49921,4150.5,2900,7050.5,1.075,0,1.075,null,null,null,657,54105.575,3524,57629.575]
[1995,50680,687,51367,4196.5,2900,7096.5,1.075,0,1.075,null,null,null,657,55534.575,3587,59121.575]
[1996,52432,687,53119,4104.5,2920,7024.5,1.075,0,1.075,null,null,null,657,57194.575,3607,60801.575]
[1997,53987,902,54889,4505.5,2920,7425.5,1.075,0,1.075,null,null,null,657,59150.575,3822,62972.575]
[1998,55857,902,56759,4792.5,2995,7787.5,6.075,0,6.075,null,null,null,657,61312.575,3897,65209.575]
[1999,58085,912,58997,5198,3309,8507,18.8,0,18.8,null,null,null,657,63958.8,4221,68179.8]
[2000,60095,968,61063,6548,4075,10623,19.025,0,19.025,null,null,null,1966,68628.025,5043,73671.025]
[2001,61438.772275802505,970.2277241974953,62409,6750.960191354861,3730.039808645139,10481,21,0,21,null,null,null,1966,70176.73246715736,4700.267532842634,74877]
[2002,63323.930180214666,1150.0698197853349,64474,9714.235745468977,4098.764254531023,13813,22,0,22,null,null,null,2007,75066.1837634139,5248.8162365861135,80315]
[2003,66493.68999749237,1204.3100025076335,67698,11291.869125306832,4838.130874693169,16130,22,0,22,null,null,null,2007,79814.5591227992,6042.440877200803,85857]
[2004,67659.15935013551,1428.8406498644906,69088,14404.518326996198,5151.481673003803,19556,27.176419213973798,1.823580786026201,29,null,null,null,2007,84096.87477780483,6582.125222195168,90679]
[2005,69472.46482351779,1587.5351764822108,71060,14626.521910777736,5143.478089222266,19770,27.176419213973798,1.823580786026201,29,null,null,null,2007,86132.18549428035,6732.814505719655,92865]
[2006,72006.44159982569,1671.5584001743086,73678,13886.244214343655,6485.7557856563435,20372,235,1.9999999999999998,237,null,null,null,2007,88135.66312682169,8159.336873178302,96294.99999999999]
[2007,73620.08453122764,3248.915468772359,76869,14205.759906213365,7023.240093786636,21229,245.20036429872496,1.7996357012750457,247,null,null,null,2007,90078.04480173973,10273.95519826027,100352]
[2008,74234.87312186978,3310.1268781302174,77545,14765.827308225218,8233.172691774784,22999,396.27156919513607,1.728430804863926,398,null,null,null,2007,91403.97199929012,11545.028000709865,102948.99999999999]
[2009,74852.60913192022,3757.3908680797717,78610,16275.502776064157,9074.497223935841,25350,600.2008487690192,1.7991512309807332,602,null,null,null,2007,93735.3127567534,12833.687243246593,106568.99999999999]
[2010,76630.7876208013,4072.212379198709,80703.00000000001,17659.232344353342,12029.767655646656,29689,925.0043080224433,1.9956919775564803,926.9999999999998,0.8,null,0.8,2007,97222.82427317709,16103.97572682292,113326.8]
[2011,78022.73877183629,4436.161228163706,82458.9,17905.63752631531,13337.189588954003,31242.827115269312,1422.9922000000001,2,1424.9922000000001,0.8,null,0.8,2007,99359.16849815159,17775.35081711771,117134.5193152693]
[2012,79673.1814433957,4620.8185566043085,84294.00000000001,18558.295970522908,14219.74776947709,32778.043739999994,1890.0742599999999,1.8,1891.8742599999998,2.082,null,2.082,2007,102130.63367391861,18842.366326081396,120973]
[2013,81212.71466495506,4805.475885044911,86018.19054999997,21426.17022,15102.305950000138,36528.47617000014,2199.766,1.9780000000000002,2201.744,2.082,2.8103400000000005,4.892340000000001,1990,106830.73288495505,19912.570175045046,126743.3030600001]
[2014,84330,4862.96219504491,89192.9621950449,21799.667579999998,16027.102420000001,37826.77,4885.671,2.01803,4887.6890300000005,6.08023,9.00025,15.08048,1990,113011.41881,20901.08289504491,133912.5017050449]
[2015,86766.0892549551,4884.1084450448925,91650.1977,21607.08492,17956.38684,39563.47176,7630.766000000001,1.9659999999982818,7632.732,6.0916484,15.25527,21.3469184,1990,118000.03182335512,22857.716555044888,140857.74837840002]
[2016,91981.79068695508,4943.20762304491,96924.99831,22101.1685,19173.70670999998,41274.875209999984,10121.976,1.96622,10123.94222,19.92155,3.83987,23.76142,1990,126214.85673695507,24122.720423044888,150337.57715999996]
[2017,95272.81134695507,5002.58878304491,100275.40012999998,21900.188591931626,19728.01964806837,41628.20823999999,12281.276640000002,1.96622,12283.242860000002,932.09076,3.2338700000000005,935.3246300000001,1990,132376.36733888672,24735.80852111328,157112.17586]
["SP-Serviço Público         PIE- Produção Independente de Energia       APE -  Autoprodução de energia"]
["SP - Public Service        PIE - Independent Energy Producer              APE - Self-producer"]
["1 Inclui metade da Usina de Itaipu"]
["1 Includes half of Itaipu Power Plant"]
["2 Usinas PIE e SP, com partes de APE, estão classificadas como SP / PIE"]
["2  Plants PIE and SP, with shares of APE, are classified as SP / PIE."]
["3 Plantas PIE, tradicionalmente APE, estão classificadas em APE."]
["3 Plants PIE, traditionally APE, are classified as APE."]
["4 Solar Fotovoltaicas"]
["4 Photovoltaic "]

{"sheet":"Tabela I.1.1","index":2,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Tabela I.1.1 - Capacidade Instalada de Itaipu"]
["Table I.1.1 - Installed Capacity of Itaipu"]
["ANO / YEAR","MW"]
[1984,1400]
[1985,2100]
[1986,4200]
[1987,6300]
[1988,8400]
[1989,10500]
[1990,11200]
["1991/2006",12600]
["2007/2017",14000]

{"sheet":"Tabela I.2","index":3,"n_rows":114,"n_cols":19,"rows_kept":114,"cut":false,"hidden":false,"merged":[[35,0,35,1],[36,0,36,1],[3,0,3,1],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,34,0],[75,0,75,1],[76,0,76,1],[112,0,112,1],[113,0,113,1],[82,0,82,1],[83,0,83,1],[84,0,84,1],[85,0,85,1],[86,0,86,1],[87,0,111,0],[44,0,44,1],[45,0,45,1],[46,0,46,1],[47,0,47,1],[48,0,48,1],[49,0,74,0]],"flags":["formulas_cached_only"]}
["Tabela I.2 Capacidade Instalada de Geração Elétrica"]
["Table I.2 Installed Capacity of Electricity Generation  "]
["Usinas em Operação / Plants in operation",null,2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017]
["UHE / Hidro",null,61554,63501.5,66460,67777.5,69630.6,72005,74937,74901,75484,77090,78347.369,79956.33955117779,81131.84413643109,84094.838,86366.478,91499.17833,94661.99466]
["PCH / Hidro",null,855,895,1151,1220,1330,1566,1820,2490,2953,3428,3896.0969390232754,4101.186511923238,4619.7684506339165,4790,4886.168299999999,4941.36157,5019.57477]
["CGH / Hidro",null,0,77,87,90,98.5,107,112,154,173,185.11765,215.53406097671854,236.47393689901511,266.38741293499385,308,397.55144,484.4584100000001,593.8307]
["EOL / Wind",null,21,22,22,29,29,237,247,398,602,926.8861999999999,1425.6,1894,2202,4888,7632.732,10123.94222,12283.242860000002]
["SOL / Solar",null,0,0,0,0,0,0,0,0,0,1,1,2,5,15,21.3469184,23.76142,935.3246300000001]
["UTE / Termo","Total",10481,13812.6,16130,19555.6,19770,20372,21229,22999,23350,29689.07422,31242.5,32778,36528,37827,39563.815909571385,41274.87520999999,41628.20824000001]
[null,"Biomassa / Biomass",{"$nulls":4},3338.38392149088,3702.355200874158,4103.189,5054.145184697088,5717.276433509134,7927.186,9027.765948194317,9922.96026137301,11601.2724871625,12341.2924,13256.624649999996,14146.949719395277,14505.317449999999]
[null,"Bagaço / Bagasse",{"$nulls":4},2298.48392149088,2644.0212008741582,3022.905,3687.0856846970873,4095.6664335091345,6183.351000000001,7213.095548194317,8095.095261373008,9435.4074871625,9881,10573.080199999997,10978.542199999982,11157.9352]
[null,"Outras / Others",{"$nulls":4},1039.8999999999996,1058.3339999999998,1080.284,1367.0595,1621.6100000000001,1743.834999999999,1814.6704,1827.865000000001,2165.864999999999,2460.2924000000003,2683.5444499999994,3168.407519395295,3347.3822499999997]
[null,"Biogás / Biogas",{"$nulls":4},19.630000000000003,20.03,20.03,32.351,44.672,68.442,70.822,79,79.594,69.857,84.13999999999999,118.63319999999999,135.1538]
[null,"Capim Elefante / Elephant Grass",{"$nulls":4},0,0,0,0,0,0,31.7,31.7,31.7,31.7,31.7,65.7,31.7]
[null,"Carvão Vegetal / Charcoal",{"$nulls":4},8,8,8,16.6,25.2,25.2,25.2,25.2,25.2,51.4,51.428999999999995,54.097,43.197]
[null,"Casca de Arroz / Rice Peels",{"$nulls":4},6.4,6.4,18.92,25.164,31.408,18.908,32.608,36.433,36.433,37.533,45.333,45.333,45.333]
[null,"Gás de Alto Forno - Biomassa / Charcoal Gas",{"$nulls":4},21.5,22.31,22.31,70,85.465,87.865,87.865,92.865,92.865,107.865,111.86505,115.26505,114.26505]
[null,"Lixívia / Black-Liquor",{"$nulls":4},782.5379999999998,785.262,794.817,970.3075,1145.798,1240.792999999999,1245.198,1235.981600000001,1529.787599999999,1785.102,1923.136,2332.95181547487,2542.616]
[null,"Óleos Vegetais / Vegetable Oil",{"$nulls":4},0,0,0,0,0,0,4.3504,4.3504,4.3504,19.110400000000002,26.9004,4.3504,4.3504]
[null,"Lenha-Resíduos de madeira e florestais / Firewood-Wood Waste",{"$nulls":4},201.832,216.332,216.207,252.637,289.067,302.627,316.927,322.335,365.935,357.725,409.04099999999994,432.07705392042544,430.767]
[null,"Fóssil / Fossil",{"$nulls":4},15809.06807850912,16035.096799125844,16278.835118500063,17097.974315302916,16753.705566490866,20373.335439243696,20818.41605180568,21444.221738626984,23589.729512837504,24148.709600000006,24960.838502697647,25549.76426066719,25452.857569091742]
[null,"Carvão Mineral / Steam Coal",{"$nulls":4},1415,1415,1415,1472.652,1530.304,1944.054,1944.054,2304.191,3389.465,3389.465,3389.4649999999997,3389.4649999999997,3323.74]
[null,"Gás de Refinaria / Refinery Gas",{"$nulls":4},281.7,281.7,281.7,281.85,282,305,305,341.6,253.8,321.26759999999996,315.56,315.56,315.56]
[null,"Gás Natural / Natural Gas",{"$nulls":4},9637.59955163603,9819.972402341584,10193.525161089694,10352.524771832826,9754.810728749962,11254.844994745006,11525.257835894214,11439.114888525995,12300.288649978887,12550,12427.73620286966,12964.558339999998,12980.311219999998]
[null,"Óleo Combustível / Fuel Oil",{"$nulls":4},1008.5955456372695,1271.3391310431318,1338.8970684276553,1514.470130907293,1564.4907710431326,2731.712454066876,3027.7945226137754,3801.21132565745,3964.5165609139785,4065.045941599454,3196.5059298279784,4020.0618232570187,4055.8249800000003]
[null,"Óleo Diesel / Diesel Oil",{"$nulls":4},3335.1729812358185,3116.085265741128,2918.712888982713,3345.4774125627955,3491.1000666977693,4006.7239904318144,3885.3096932976923,3427.104524443542,3550.6593019446373,3822.93105840055,5631.57137000001,4824.638431606268,4736.596589999999]
[null,"Óleo Ultraviscoso / Viscous Oil",{"$nulls":4},131,131,131,131,131,131,131,131,131,null,null,0,0]
[null,"Outras¹ / Others¹",{"$nulls":15},35.48066580390409,40.824779091743174]
[null,"Efluentes Industriais / Industrial Effluent",{"$nulls":4},622.548,634.548,846.9679999999998,846.8805,879.018,1388.418,1396.318,1410.818,1336.9979999999998,1336.9979999999996,1346.352756873749,1578.1612299375186,1578.5332209082712]
[null,"Efluente Gasoso² / Gaseous Effluent²",{"$nulls":4},17.3,17.3,213.82,212.57,211.32,211.32,211.32,211.32,162.1,162.1,160.35507939024438,175.6969428178808,172.06893378863344]
[null,"Enxofre / Sulfur",{"$nulls":4},31.188,43.188,54.688,55.688,56.688,56.688,56.688,59.688,59.688,59.688,71.188,71.188,71.188]
[null,"Gás de Alto Forno / Blast Furnace Gas",{"$nulls":4},163.44,163.44,167.84,168.0025,200.39000000000001,206.78999999999996,211.69,211.69,215.69,215.68999999999969,216.00967748350467,422.47628711963773,422.4762871196378]
[null,"Gás de Processo / Process Gas",{"$nulls":4},132.42,132.42,132.42,132.42,132.42,635.42,638.42,649.92,674.42,674.42,673.7,653.7,657.7]
[null,"Gás Siderúrgico / Steel Gas",{"$nulls":4},278.2,278.2,278.2,278.2,278.2,278.2,278.2,278.2,225.1,225.1,225.1,255.1,255.1]
[null,"Fontes Desconhecidas",{"$nulls":16},91.5]
["UTN / Nuclear",null,1966,2007,2007,2007,2007,2007,2007,2007,2007,2007,2007,2007,1990,1990,1990,1990,1990]
["Total",null,74877,80315.1,85857,90679.1,92865.1,96294,100352,102949,104569,113327.07806999999,117135.1,120975.00000000004,126743,133912.838,140858.09256797138,150337.57716,157112.17586000002]
[null,"¹ Inclui Alcatrão/ Includes TAR"]
[null,"² inclui calor de processo"]
[]
[]
["Tabela I.2 Capacidade Instalada de Geração Elétrica"]
["Table I.2 Installed Capacity of Electricity Generation  "]
["Usinas em Operação / Plants in operation",null,2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016]
["UHE / Hidro",null,61554,63501.5,66460,67777.5,69630.6,72005,74937,74901,75484,77090,78347.369,79956.33955117779,81131.84413643109,84094.838,86366.478,91499.17833]
["PCH / Hidro",null,855,895,1151,1220,1330,1566,1820,2490,2953,3428,3896.0969390232754,4101.186511923238,4619.7684506339165,4790,4886.168299999999,4941.36157]
["CGH / Hidro",null,0,77,87,90,98.5,107,112,154,173,185.11765,215.53406097671854,236.47393689901511,266.38741293499385,308,397.55144,484.4584100000001]
["EOL / Wind",null,21,22,22,29,29,237,247,398,602,926.8861999999999,1425.6,1894,2202,4888,7632.732,10123.94222]
["SOL / Solar",null,0,0,0,0,0,0,0,0,0,1,1,2,5,15,21.3469184,23.76142]
["UTE / Termo","Total",10481,13812.6,16130,19555.6,19770,20372,21229,22999,23350,29689.07422,31242.5,32778,36528,37827,39563.815909571385,41274.87520999999]
[null,"Biomassa / Biomass",{"$nulls":4},3338.38392149088,3702.355200874158,4103.189,5054.145184697088,5717.276433509134,7927.186,9027.765948194317,9922.96026137301,11601.2724871625,12341.2924,13256.624649999996,14146.949719395277]
[null,"Bagaço / Bagasse",{"$nulls":4},2298.48392149088,2644.0212008741582,3022.905,3687.0856846970873,4095.6664335091345,6183.351000000001,7213.095548194317,8095.095261373008,9435.4074871625,9881,10573.080199999997,10978.542199999982]
[null,"Outras / Others",{"$nulls":4},1039.8999999999996,1058.3339999999998,1080.284,1367.0595,1621.6100000000001,1743.834999999999,1814.6704,1827.865000000001,2165.864999999999,2460.2924000000003,2683.5444499999994,3168.407519395295]
[null,"Biogás / Biogas",{"$nulls":4},19.630000000000003,20.03,20.03,32.351,44.672,68.442,70.822,79,79.594,69.857,84.13999999999999,118.63319999999999]
[null,"Capim Elefante / Elephant Grass",{"$nulls":10},31.7,31.7,31.7,31.7,31.7,65.7]
[null,"Carvão Vegetal / Charcoal",{"$nulls":4},8,8,8,16.6,25.2,25.2,25.2,25.2,25.2,51.4,51.428999999999995,54.097]
[null,"Casca de Arroz / Rice Peels",{"$nulls":4},6.4,6.4,18.92,25.164,31.408,18.908,32.608,36.433,36.433,37.533,45.333,45.333]
[null,"Gás de Alto Forno - Biomassa / Charcoal Gas",{"$nulls":4},21.5,22.31,22.31,70,85.465,87.865,87.865,92.865,92.865,107.865,111.86505,115.26505]
[null,"Lixívia / Black-Liquor",{"$nulls":4},782.5379999999998,785.262,794.817,970.3075,1145.798,1240.792999999999,1245.198,1235.981600000001,1529.787599999999,1785.102,1923.136,2332.95181547487]
[null,"Óleos Vegetais / Vegetable Oil",{"$nulls":10},4.3504,4.3504,4.3504,19.110400000000002,26.9004,4.3504]
[null,"Lenha-Resíduos de madeira / Firewood-Wood Waste",{"$nulls":4},201.832,216.332,216.207,252.637,289.067,302.627,316.927,322.335,365.935,357.725,409.04099999999994,432.07705392042544]
[null,"Fóssil / Fossil",{"$nulls":4},15809.06807850912,16035.096799125844,16278.835118500063,17097.974315302916,16753.705566490866,20373.335439243696,20818.41605180568,21444.221738626984,23589.729512837504,24148.709600000006,24960.838502697647,25549.76426066719]
[null,"Carvão Mineral / Steam Coal",{"$nulls":4},1415,1415,1415,1472.652,1530.304,1944.054,1944.054,2304.191,3389.465,3389.465,3389.4649999999997,3389.4649999999997]
[null,"Gás de Refinaria / Refinery Gas",{"$nulls":4},281.7,281.7,281.7,281.85,282,305,305,341.6,253.8,321.26759999999996,315.56,315.56]
[null,"Gás Natural / Natural Gas",{"$nulls":4},9637.59955163603,9819.972402341584,10193.525161089694,10352.524771832826,9754.810728749962,11254.844994745006,11525.257835894214,11439.114888525995,12300.288649978887,12550,12427.73620286966,12964.558339999998]
[null,"Óleo Combustível / Fuel Oil",{"$nulls":4},1008.5955456372695,1271.3391310431318,1338.8970684276553,1514.470130907293,1564.4907710431326,2731.712454066876,3027.7945226137754,3801.21132565745,3964.5165609139785,4065.045941599454,3196.5059298279784,4020.0618232570187]
[null,"Óleo Diesel / Diesel Oil",{"$nulls":4},3335.1729812358185,3116.085265741128,2918.712888982713,3345.4774125627955,3491.1000666977693,4006.7239904318144,3885.3096932976923,3427.104524443542,3550.6593019446373,3822.93105840055,5631.57137000001,4824.638431606268]
[null,"Óleo Ultraviscoso / Viscous Oil",{"$nulls":4},131,131,131,131,131,131,131,131,131]
[null,"Outras¹ / Others¹",{"$nulls":15},35.48066580390409]
[null,"Efluentes Industriais / Industrial Effluent",{"$nulls":4},622.548,634.548,846.9679999999998,846.8805,879.018,1388.418,1396.318,1410.818,1336.9979999999998,1336.9979999999996,1346.352756873749,1578.1612299375186]
[null,"Efluente Gasoso² / Gaseous Effluent²",{"$nulls":4},17.3,17.3,213.82,212.57,211.32,211.32,211.32,211.32,162.1,162.1,160.35507939024438,175.6969428178808]
[null,"Enxofre / Sulfur",{"$nulls":4},31.188,43.188,54.688,55.688,56.688,56.688,56.688,59.688,59.688,59.688,71.188,71.188]
[null,"Gás de Alto Forno / Blast Furnace Gas",{"$nulls":4},163.44,163.44,167.84,168.0025,200.39000000000001,206.78999999999996,211.69,211.69,215.69,215.68999999999969,216.00967748350467,422.47628711963773]
[null,"Gás de Processo / Process Gas",{"$nulls":4},132.42,132.42,132.42,132.42,132.42,635.42,638.42,649.92,674.42,674.42,673.7,653.7]
[null,"Gás Siderúrgico / Steel Gas",{"$nulls":4},278.2,278.2,278.2,278.2,278.2,278.2,278.2,278.2,225.1,225.1,225.1,255.1]
["UTN / Nuclear",null,1966,2007,2007,2007,2007,2007,2007,2007,2007,2007,2007,2007,1990,1990,1990,1990]
["Total",null,74877,80315.1,85857,90679.1,92865.1,96294,100352,102949,104569,113327.07806999999,117135.1,120975.00000000004,126743,133912.838,140858.09256797138,150337.57716]
[null,"¹ Inclui Alcatrão/ Includes TAR"]
[null,"² inclui calor de processo"]
[]
[]
["Usinas em Operação / Plants in operation",null,2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015]
["UHE / Hidro",null,61554,63501.5,66460,67777.5,69630.6,72005,74937,74901,75484,77090,78347.369,79956.33955117779,81131.84413643109,84094.838,86366.478]
["PCH / Hidro",null,855,895,1151,1220,1330,1566,1820,2490,2953,3428,3896.0969390232754,4101.186511923238,4619.7684506339165,4790,4886.168299999999]
["CGH / Hidro",null,0,77,87,90,98.5,107,112,154,173,185.11765,215.53406097671854,236.47393689901511,266.38741293499385,308,397.55144]
["EOL / Wind",null,21,22,22,29,29,237,247,398,602,926.8861999999999,1425.6,1894,2202,4888,7632.732]
["SOL / Solar",null,0,0,0,0,0,0,0,0,0,1,1,2,5,15,21.3469184]
["UTE / Termo","Total",10481,13812.6,16130,19555.6,19770,20372,21229,22999,23350,29689.07422,31242.5,32778,36528,37827,39563.81590957139]
[null,"Biomassa / Biomass",{"$nulls":4},3338.38392149088,3702.355200874158,4103.189,5054.145184697088,5717.276433509134,7927.186,9027.765948194317,9922.96026137301,11601.2724871625,12341.2924,13256.624649999996]
[null,"Bagaço / Bagasse",{"$nulls":4},2298.48392149088,2644.0212008741582,3022.905,3687.0856846970873,4095.6664335091345,6183.351000000001,7213.095548194317,8095.095261373008,9435.4074871625,9881,10573.080199999997]
[null,"Outras / Others",{"$nulls":4},1039.8999999999996,1058.3339999999998,1080.284,1367.0595,1621.6100000000001,1743.834999999999,1814.6704,1827.865000000001,2165.864999999999,2460.2924000000003,2683.5444499999994]
[null,"Biogás / Biogas",{"$nulls":4},19.630000000000003,20.03,20.03,32.351,44.672,68.442,70.822,79,79.594,69.857,84.13999999999999]
[null,"Capim Elefante / Elephant Grass",{"$nulls":4},0,0,0,0,0,0,31.7,31.7,31.7,31.7,31.7]
[null,"Carvão Vegetal / Charcoal",{"$nulls":4},8,8,8,16.6,25.2,25.2,25.2,25.2,25.2,51.4,51.428999999999995]
[null,"Casca de Arroz / Rice Peels",{"$nulls":4},6.4,6.4,18.92,25.164,31.408,18.908,32.608,36.433,36.433,37.533,45.333]
[null,"Gás de Alto Forno - Biomassa / Charcoal Gas",{"$nulls":4},21.5,22.31,22.31,70,85.465,87.865,87.865,92.865,92.865,107.865,111.86505]
[null,"Lixívia / Black-Liquor",{"$nulls":4},782.5379999999998,785.262,794.817,970.3075,1145.798,1240.792999999999,1245.198,1235.981600000001,1529.787599999999,1785.102,1923.136]
[null,"Óleos Vegetais / Vegetable Oil",{"$nulls":4},0,0,0,0,0,0,4.3504,4.3504,4.3504,19.110400000000002,26.9004]
[null,"Resíduos de madeira / Wood Waste",{"$nulls":4},201.832,216.332,216.207,252.637,289.067,302.627,316.927,322.335,365.935,357.725,409.04099999999994]
[null,"Fóssil / Fossil",{"$nulls":4},15809.06807850912,16035.096799125844,16278.835118500063,17097.974315302916,16753.705566490866,20373.335439243696,20818.41605180568,21444.221738626984,23589.729512837504,24148.709600000002,24960.838502697647]
[null,"Carvão Mineral / Steam Coal",{"$nulls":4},1415,1415,1415,1472.652,1530.304,1944.054,1944.054,2304.191,3389.465,3389.465,3389.4649999999997]
[null,"Gás de Refinaria / Refinery Gas",{"$nulls":4},281.7,281.7,281.7,281.85,282,305,305,341.6,253.8,321.26759999999996,315.56]
[null,"Gás Natural / Natural Gas",{"$nulls":4},9637.59955163603,9819.972402341584,10193.525161089694,10352.524771832826,9754.810728749962,11254.844994745006,11525.257835894214,11439.114888525995,12300.288649978887,12550,12427.73620286966]
[null,"Óleo Combustível / Fuel Oil",{"$nulls":4},1008.5955456372695,1271.3391310431318,1338.8970684276553,1514.470130907293,1564.4907710431326,2731.712454066876,3027.7945226137754,3801.21132565745,3964.5165609139785,4065.045941599454,4140.8920698279835]
[null,"Óleo Diesel / Diesel Oil",{"$nulls":4},3335.1729812358185,3116.085265741128,2918.712888982713,3345.4774125627955,3491.1000666977693,4006.7239904318144,3885.3096932976923,3427.104524443542,3550.6593019446373,3691.931058400546,4556.185230000001]
[null,"Óleo Ultraviscoso / Viscous Oil",{"$nulls":4},131,131,131,131,131,131,131,131,131,131,131]
[null,"Efluentes Industriais / Industrial Effluent",{"$nulls":4},622.548,634.548,846.9679999999998,846.8805,879.018,1388.418,1396.318,1410.818,1336.9979999999998,1336.9979999999996,1346.352756873749]
[null,"Efluente Gasoso / Gaseous Effluent",{"$nulls":4},17.3,17.3,213.82,212.57,211.32,211.32,211.32,211.32,162.1,162.1,160.35507939024438]
[null,"Enxofre / Sulfur",{"$nulls":4},31.188,43.188,54.688,55.688,56.688,56.688,56.688,59.688,59.688,59.688,71.188]
[null,"Gás de Alto Forno / Blast Furnace Gas",{"$nulls":4},163.44,163.44,167.84,168.0025,200.39000000000001,206.78999999999996,211.69,211.69,215.69,215.68999999999969,216.00967748350467]
[null,"Gás de Processo / Process Gas",{"$nulls":4},132.42,132.42,132.42,132.42,132.42,635.42,638.42,649.92,674.42,674.42,673.7]
[null,"Gás Siderúrgico / Steel Gas",{"$nulls":4},278.2,278.2,278.2,278.2,278.2,278.2,278.2,278.2,225.1,225.1,225.1]
["UTN / Nuclear",null,1966,2007,2007,2007,2007,2007,2007,2007,2007,2007,2007,2007,1990,1990,1990]
["Total",null,74877,80315.1,85857,90679.1,92865.1,96294,100352,102949,104569,113327.07806999999,117135.1,120975.00000000004,126743,133912.838,140858.09256797138]

{"sheet":"Tabela I.3","index":4,"n_rows":52,"n_cols":2,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Tabela I.3 - Capacidade Instalada de Refino de Petróleo"]
["Table I.3 - Installed Capacity of Oil Refining"]
["ANO / YEAR","m³/dia (day)"]
[1974,164200]
[1975,166700]
[1976,165700]
[1977,185800]
[1978,201100]
[1979,201100]
[1980,233100]
[1981,233300]
[1982,238200]
[1983,240100]
[1984,240100]
[1985,240100]
[1986,240100]
[1987,240100]
[1988,234890]
[1989,241040]
[1990,241040]
[1991,241750]
[1992,241680]
[1993,239080]
[1994,246580]
[1995,247880]
[1996,249461]
[1997,278198]
[1998,281096]
[1999,285475]
[2000,294025]
[2001,294025]
[2002,294690]
[2003,304523]
[2004,304523]
[2005,304618]
[2006,304618]
[2007,307563]
[2008,325050]
[2009,332703]
[2010,332703]
[2011,333175]
[2012,334433]
[2013,334433]
[" 20141",364409]
[2015,374209.0808064772]
["2016",380130.204]
["2017",380130.204]
["1 1º trem da refinaria RNEST entrou em operação em 6 dezembro de 2014, conforme Autorização ANP (de operação) nº 506/2014"]
["1 The refinery RNEST started operation on  6 december of 2014,  Autorized by ANP (operation) nº 506/2014"]
[]
["Fonte:","RELATÓRIO DO MERCADO DE DERIVADOS DE PETRÓLEO - MME"]
[null,"http://www.mme.gov.br/web/guest/secretarias/petroleo-gas-natural-e-combustiveis-renovaveis/publicacoes/relatorio-mensal-do-mercado-de-derivados-de-petroleo"]

{"sheet":"aux I.1","index":6,"n_rows":52,"n_cols":15,"rows_kept":52,"cut":false,"hidden":true,"merged":[[9,12,9,14],[9,0,10,0],[9,7,9,9]],"flags":["formulas_cached_only"]}
[null,null,null,"Retorna ao Índice"]
[]
[]
[]
[]
[]
[]
["TABLE I.1"]
["INSTALLED CAPACITY OF ELECTRIC ENERGY GENERATION ",{"$nulls":13},"MW"]
["YEAR","                      HYDRO (1)",null,null,"                       THERMO",null,null,"WIND",null,null,"THERMO E WIND","NUCLEAR","TOTAL"]
[null,"SP / PIE (2)","APE (3)","TOTAL","SP / PIE","APE","TOTAL","SP / PIE","APE","TOTAL",null,"SP","SP / PIE","APE","TOTAL"]
[1974,13224,500,13724,2489,1920,4409,0,0,0,4409,0,15713,2420,18133]
[1975,15815,501,16316,2436,2216,4652,0,0,0,4652,0,18251,2717,20968]
[1976,17343,561,17904,2457,2223,4680,0,0,0,4680,0,19800,2784,22584]
[1977,18835,561,19396,2729,2214,4943,0,0,0,4943,0,21564,2775,24339]
[1978,21104,561,21665,3048,2259,5307,0,0,0,5307,0,24152,2820,26972]
[1979,23667,568,24235,3573,2411,5984,0,0,0,5984,0,27240,2979,30219]
[1980,27081,568,27649,3484,2339,5823,0,0,0,5823,0,30565,2907,33472]
[1981,30596,577,31173,3655,2441,6096,0,0,0,6096,0,34251,3018,37269]
[1982,32542,614,33156,3687,2503,6190,0,0,0,6190,0,36229,3117,39346]
[1983,33556,622,34178,3641,2547,6188,0,0,0,6188,0,37197,3169,40366]
[1984,34301,622,34923,3626,2547,6173,0,0,0,6173,0,37927,3169,41096]
[1985,36453,624,37077,3708,2665,6373,0,0,0,6373,657,40818,3289,44107]
[1986,37162,624,37786,3845,2665,6510,0,0,0,6510,657,41664,3289,44953]
[1987,39693,636,40329,3910,2665,6575,0,0,0,6575,657,44260,3301,47561]
[1988,41583,645,42228,4025,2665,6690,0,0,0,6690,657,46265,3310,49575]
[1989,44172,624,44796,4007,2665,6672,0,0,0,6672,657,48836,3289,52125]
[1990,44934,624,45558,4170,2665,6835,0,0,0,6835,657,49761,3289,53050]
[1991,45992,624,46616,4203,2665,6868,0,0,0,6868,657,50852,3289,54141]
[1992,47085,624,47709,4018.5,2665,6683.5,0.075,0,0.075,6683.575,657,51760.575,3289,55049.575]
[1993,47967,624,48591,4127.5,2847,6974.5,0.075,0,0.075,6974.575,657,52751.575,3471,56222.575]
[1994,49297,624,49921,4150.5,2900,7050.5,1.075,0,1.075,7051.575,657,54105.575,3524,57629.575]
[1995,50680,687,51367,4196.5,2900,7096.5,1.075,0,1.075,7097.575,657,55534.575,3587,59121.575]
[1996,52432,687,53119,4104.5,2920,7024.5,1.075,0,1.075,7025.575,657,57194.575,3607,60801.575]
[1997,53987,902,54889,4505.5,2920,7425.5,1.075,0,1.075,7426.575,657,59150.575,3822,62972.575]
[1998,55857,902,56759,4792.5,2995,7787.5,6.075,0,6.075,7793.575,657,61312.575,3897,65209.575]
[1999,58085,912,58997,5198,3309,8507,18.8,0,18.8,8525.8,657,63958.8,4221,68179.8]
[2000,60095,968,61063,6548,4075,10623,19.025,0,19.025,10642.025,2007,68669.025,5043,73712.025]
[2001,61551,972,62523,7540,4166,11706,19.025,0,19.025,11725.025,2007,71117.025,5138,76255.025]
[2002,64146,1165,65311,10632,4486,15118,22.025,0,22.025,15140.025,2007,76807.025,5651,82458.025]
[2003,66587,1206,67793,11693,5010,16703,26.825,1.8,28.625,16731.625,2007,80313.825,6217.8,86531.625]
[2004,67572,1427,68999,14529,5196,19725,26.825,1.8,28.625,19753.625,2007,84134.825,6624.8,90759.625]
[2005,69274,1583,70857,14992,5272,20264,26.825,1.8,28.625,20292.625,2007,86299.825,6856.8,93156.625]
[2006,71767,1666,73433,14285,6672,20957,235.05,1.8,236.85,21193.85,2007,88294.05,8339.8,96633.85]
[2007,73622,3249,76871,14270,7055,21325,245.25,1.8,247.05,21572.05,2007,90144.25,10305.8,100450.05]
[2008,74546,3742,78288,15291,7961,23252,412.68,1.8,414.48,23666.48,2007,92256.68,11704.8,103961.48]
[2009,75586.7,3704.4,79291.1,15291.356020000003,9023.560373465409,24314.916393465413,600.484,1.8,602.284,24917.200393465413,2007,93485.54002000001,12729.760373465408,106215.30039346543]
["SP - Public Service        PIE - Independent Energy Producer      APE - Self-producer"]
[]
["(1) It includes half of Itaipu Power Plant"]
["(2) Plants  PIE and SP, with shares of APE, are classified as SP / PIE."]
["(3) Plants PIE, traditionally APE, are classified as APE."]

{"sheet":"auxI.2","index":7,"n_rows":19,"n_cols":4,"rows_kept":19,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"Retorna ao Índice"]
[]
[]
[]
[]
[]
[]
["TABLE I.2"]
["INSTALLED CAPACITY IN ITAIPU"]
["YEAR","MW"]
[1984,1400]
[1985,2100]
[1986,4200]
[1987,6300]
[1988,8400]
[1989,10500]
[1990,11200]
[1991,12600]
[2007,14000]

{"sheet":"auxI.3","index":8,"n_rows":47,"n_cols":3,"rows_kept":47,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"Retorna ao Índice"]
[]
[]
[]
[]
[]
[]
["TABLE I.3"]
["INSTALLED CAPACITY OF OIL REFINING IN DEC/31(*)"]
["YEAR","m³ / o-d 1"]
[1974,164200]
[1975,166700]
[1976,165700]
[1977,185800]
[1978,201100]
[1979,201100]
[1980,233100]
[1981,233300]
[1982,238200]
[1983,240100]
[1984,240100]
[1985,240100]
[1986,240100]
[1987,240100]
[1988,234890]
[1989,241040]
[1990,241040]
[1991,241750]
[1992,241680]
[1993,239080]
[1994,246580]
[1995,247880]
[1996,249461]
[1997,278198]
[1998,281096]
[1999,285475]
[2000,294025]
[2001,294025]
[2002,294690]
[2003,304523]
[2004,304523]
[2005,304618]
[2006,304618]
[2007,307563]
[2008,325050]
[2009,332703]
[2010,332703]